**©2019 Eliminating Lighting** all rights reserved. Information, specifications, diagrams, images, and instructions herein are subject to change without notice. Eliminator Lighting logo and identifying product names and numbers herein are trademarks of Eliminator Lighting. Copyright protection claimed includes all forms and matters of copyrightable materials and information now allowed by statutory or judicial law or hereinafter granted. Product names used in this document may be trademarks or registered trademarks of their respective companies and are hereby acknowledged. All non- Eliminator Lighting brands and product names are trademarks or registered trademarks of their respective companies. **Eliminator Lighting** and all affiliated companies hereby disclaim any and all liabilities for property, equipment, building, and electrical damages, injuries to any persons, and direct or indirect economic loss associated with the use or reliance of any information contained within this document, and/or as a result of the improper, unsafe, insufficient and negligent assembly, installation, rigging, and operation of this product.

**Eliminator Lighting USA** 6122 S. Eastern Ave. Los Angeles, CA. 90040

323-948-0480 | Fax 888-287-5224 **|** www.eliminatorlighting.com | info@eliminatorlighting.com

**Eliminator Lighting Customer Support**

323-213-4592 | Fax 888-287-5224 **|** support@eliminatorlighting.com

**UNPACKING** This product has been thoroughly tested and has been shipped in perfect condition. Carefully check the shipping carton for damage that may have occurred during shipping. If the carton appears to be damaged, carefully inspect your product for damage and be sure all accessories necessary to assemble the product have arrived intact. In the event damage has been found or parts are missing, please contact our customer support team for further instructions.

Please do not return this product to your dealer without first contacting customer support at the number listed below. Please do not discard the shipping carton in the trash. Please recycle whenever possible.

**LIMITED WARRANTY (USA ONLY)**

A. Eliminator Lighting, an ADJ Products, LLC brand, hereby warrants, to the original purchaser, ADJ Products, LLC products to be free of manufacturing defects in material and workmanship for a prescribed period from the date of purchase (see specific warranty period on reverse). This warranty shall be valid only if the product is purchased within the United States of America, including possessions and territories. It is the owner’s responsibility to establish the date and place of purchase by acceptable evidence, at the time service is sought.

B. For warranty service you must obtain a Return Authorization number (RA#) before sending back the product–please contact ADJ Products, LLC Service Department at 800-322-6337. Send the product only to the ADJ Products, LLC factory. All shipping charges must be pre-paid. If the requested repairs or service (including parts replacement) are within the terms of this warranty, ADJ Products, LLC will pay return shipping charges only to a designated point within the United States. If the entire instrument is sent, it must be shipped in its original package. No accessories should be shipped with the product. If any accessories are shipped with the product, ADJ Products, LLC shall have no liability whatsoever for loss of or damage to any such accessories, or for the safe return thereof.

C. This warranty is void if the serial number has been altered or removed; if the product is modified in any manner which ADJ Products, LLC concludes, after inspection, affects the reliability of the product; if the product has been repaired or serviced by anyone other than the ADJ Products, LLC factory unless prior written authorization was issued to purchaser by ADJ Products, LLC; if the product is damaged because not properly maintained as set forth in the instruction manual.

D. This is not a service contract, and this warranty does not include maintenance, cleaning or periodic check-up. During the period specified above, ADJ Products, LLC will replace defective parts at its expense with new or refurbished parts, and will absorb all expenses for warranty service and repair labor by reason of defects in material or workmanship. The sole responsibility of ADJ Products, LLC under this warranty shall be limited to the repair of the product, or replacement thereof, including parts, at the sole discretion of ADJ Products, LLC.  All products covered by this warranty were manufactured after August 15, 2012, and bear identifying marks to that effect.

E. ADJ Products, LLC reserves the right to make changes in design and/or improvements upon its products without any obligation to include these changes in any products theretofore manufactured. No warranty, whether expressed or implied, is given or made with respect to any accessory supplied with products described above. Except to the extent prohibited by applicable law, all implied warranties made by ADJ Products, LLC in connection with this product, including warranties of merchantability or fitness, are limited in duration to the warranty period set forth above. And no warranties, whether expressed or implied, including warranties of merchantability or fitness, shall apply to this product after said period has expired. The consumer’s and/or Dealer’s sole remedy shall be such repair or replacement as is expressly provided above; and under no circumstances shall ADJ Products, LLC be liable for any loss or damage, direct or consequential, arising out of the use of, or inability to use, this product.

This warranty is the only written warranty applicable to Eliminator Lighting, an ADJ Products, LLC brand, and supersedes all prior warranties and written descriptions of warranty terms and conditions heretofore published.

**MANUFACTURER’S LIMITED WARRANTY PERIODS:**

**All Eliminator Lighting products (except laser diodes) = 1-year (365 days)** Limited Warranty (Such as: Special Effect Lighting, Intelligent Lighting, UV lighting, Strobes, Fog Machines, Bubble Machines, Mirror Balls, Par Cans, Trussing, Lighting Stands etc., excluding lamps)

**Laser Products = 1 Year (365 Days)** Limited Warranty (excluding laser diodes which have a 6 month limited warranty)

**Batteries = 180 Day** Limited Warranty

To register your Eliminator Lighting product online, please click here to the ADJ Warranty Registration Page: https://www.adj.com/portal/user/register/

**WARRANTY RETURNS**

All returned service items whether under warranty or not, must be freight pre-paid and accompany a return authorization (R.A.) number. The R.A. number must be clearly written on the outside of the return package. A brief description of the problem as well as the R.A. number must also be written down on a piece of paper and included in the shipping container. If the unit is under warranty, you must provide a copy of your proof of purchase invoice. Items returned without a R.A. number clearly marked on the outside of the package will be refused and returned at customer’s expense. You may obtain a R.A. number by contacting customer support.

**ELIMINATOR LIGHTING BLACK 24**

**TECHNICAL SPECIFICATIONS**

**Lamp Type:** 24-inch Bi-Pin (T12) 20-Watt

**Control:** On/Off Switch

**Included Items:** Fixture, 3-Foot Attached Power Cord, and Lamp

**Lamp:** LL-F20BLB

**Dimensions (L x W x H):** 5” x 3” x 25” (127mm x 76.2mm x 635mm)

**Weight:** 2.0 lbs. (0.9 kg)

**Ultra Violet Wavelength:** 365nm

**ELIMINATOR LIGHTING BLACK 24**

**SAFETY GUIDELINES**

**INDOOR / DRY LOCATIONS USE ONLY!**

**KEEP FLAMMABLE MATERIALS AWAY FROM FIXTURE!**

**DO NOT EXPOSE FIXTURE TO RAIN AND/OR MOISTURE!**

**DO NOT PLUG FIXTURE INTO A DIMMER PACK!**

**DO NOT OPERATE FIXTURE IF THE POWER CORD IS FRAYED, CRIMPED, OR DAMAGED.**

**THERE ARE NO USER SERVICEABLE PARTS INSIDE THIS FIXTURE!**

**DO NOT ATTEMPT ANY REPAIRS YOURSELF; DOING SO VOIDS YOUR WARRANTY.**

**DAMAGE RESULTING FROM MODIFICATIONS AND/OR DISREGARD OF SAFETY GUIDELINES VOIDS THE WARRANTY.**

**UNPLUG FIXTURE POWER BEFORE REPLACING THE LAMP!**

**NEVER TOUCH FIXTURE OR LAMP DURING OPERATION, AS IT MAY BE HOT!**

**TURN OFF FIXTURE AND ALLOW TO COOL APPROXIMATELY 15 MINUTES BEFORE REPLACING LAMP!**

**RISK GROUP 3 - RISK OF EXPOSURE TO ULTRAVIOLET RADIATION!**

**FIXTURE EMITS HIGH INTENSITY WAVELENGTH OF ULTRAVIOLET LIGHT.**

**WEAR PROPER EYE AND SKIN PROTECTION.**

**AVOID PROLONGED PERIODS OF EXPOSURE TO ULTRAVIOLET LIGHT.**

**AVOID WEARING WHITE COLOR CLOTHING AND/OR USING UV PAINTS ON SKIN.**

**AVOID DIRECT EYE AND/OR SKIN EXPOSURE AT DISTANCES LESS THAN 11 FEET.**

**DO NOT OPERATE FIXTURE WITH DAMAGED/MISSING EXTERNAL COVERS.**

**DO NOT LOOK DIRECTLY INTO THE UV LIGHT AND/OR VIEW DIRECTLY WITH OPTICAL INSTRUMENTS THAT MAY CONCENTRATE THE UV LIGHT/RADIATION OUTPUT. INDIVIDUALS SUFFERING FROM A RANGE OF EYE CONDITIONS, SUNLIGHT EXPOSURE DISORDERS, OR INDIVIDUALS USING PHOTOSENSITIVE MEDICATION, MAY RECEIVE DISCOMFORT IF EXPOSED TO THE ULTRAVIOLET LIGHT EMITTED FROM THE FIXTURE.**

**TROUBLE SHOOTING**

**Light does not turn ON, flickers, or is not ON 100%.**

Check if the fixture power cord is connected to a suitable power source.

Check if the fixture power switch is in the ON position.

Power OFF the fixture then carefully check if the bulb is properly installed/seated in the fixture.

Check if both contact pins on both ends of the bulb are inserted correctly into the fixture.

The bulb may have shifted during shipping, during installation of the fixture, or while in use.

The bulb may need to be replaced. Replace with ADJ bulb ONLY. Contact ADJ Service for support or questions.

**BULB REPLACEMENT ADJ# LLF20-BLB**

1. Power fixture OFF and disconnect power cord from power source and wait 15 minutes to allow the bulb to cool.

2. Using both hands, gently twist the bulb counter-clockwise to remove.

3. Using both hands, gently align contact pins on both ends of the bulb to the fixture.

4. Insert the bulb gently into the fixture, then turn clockwise to secure in place.

**CLEANING**

Power fixture OFF and let cool for 15 minutes. Use a soft cloth to clean dust or debris from bulb and fixture. Routine cleaning is recommended every 30 days to ensure the best performance.